Convert delay 30 milliseconds to samples, initialize write index with this value. Write incoming data into buffer. Generate sine wave of 0.2 Hz (LFO), use this sine wave to calculate read index. Use interpolation to avoid artifacts (distortions) . Add original signal and variable time delayed signal produced by previous structure to produce chorus effect output signal.