Spectrum of AM signal is a copy of spectrum of input signal mirrored around carrier frequency i.e. frequency of cosine signal (in this case f0 = 1000Hz)



